Roofing Requirements:

1. Wood shakes, wood shingles or synthetic shake shingles with the appearance, color, texture and thickness or natural wood shakes.
2. CertainTeed Presidential, Tamko Vintage, IKO Armourshake, GAF Grand Sequoia, GAF Camelot, or like Premium Grade shingles. Colors need to be earth tone and approved by the architectural committee.
3. Any material pre-approved by the architectural committee; provided, however, that the architectural committee shall only approve of materials similar in appearance, texture and quality as these materials enumerated in items (1) and (2) above.